Cyclades multiport serial boards [include/linux/cyclades.h]
`CYGETMON` |
`CYGETTHRESH` |
`CYSETTHRESH` |
`CYGETDEFTHRESH` |
`CYSETDEFTHRESH` |
`CYGETTIMEOUT` |
`CYSETTIMEOUT` |
`CYGETDEFTIMEOUT` |
`CYSETDEFTIMEOUT` |
`CYSETRFLOW` |
`CYGETRFLOW` |
`CYSETRTSDTR_INV` |
`CYGETRTSDTR_INV` |
`CYZSETPOLLCYCLE` |
`CYZGETPOLLCYCLE` |
`CYGETCD1400VER` |
`CYGETCARDINFO` |
`CYSETWAIT` |
`CYGETWAIT` |
These IOCTLs will also work with Motorola MVME166/7 board serial ports driver which is heavily based on Cyclades driver.