AX.25 Protocol [include/linux/ax25.h]
`SIOCAX25GETUID` | Get a UID information from the uid/call map table. `*to be documented*`
`SIOCAX25ADDUID` | Add a UID to the uid/call map table. `*to be documented*`
`SIOCAX25DELUID` | Delete a UID from the uid/call map table. `*to be documented*`
`SIOCAX25NOUID` | Set the default policy (default/bar). `*to be documented*`
`SIOCAX25OPTRT` | `*to be documented*`
`SIOCAX25CTLCON` | `*to be documented*`
`SIOCAX25GETINFOOLD` | `*to be documented*`
`SIOCAX25ADDFWD` | `*to be documented*`
`SIOCAX25DELFWD` | `*to be documented*`
`SIOCAX25DEVCTL` | `*to be documented*`
`SIOCAX25GETINFO` | `*to be documented*`