sys_rt_sigpending [kernel/signal.c]
Returns the set of "realtime" signals that are pending for delivery to the calling thread (i.e., the signals which have been raised while blocked). Arguments
eax | 176
ebx | Pointer to a dword which will receive the mask of pending signals.
ecx | Size of the sigset_t (see include/asm-i386/signal.h).
Return values If the system call succeeds the return value is 0. If the system call fails the return value is one of the following errno values:
`-EFAULT` | `ebx points to memory which is not a valid part of the process address space.`
Remarks n/a Compatibility n/a